**No. 2216TimberCraft***®* **Full-Round Log Seat**

Full-Round Log Seat shall be TimberCraft*®* series model No. 2216, in the length and quantity shown on the bill of materials or the project drawings. Manufacturer, Columbia Cascade Company, 1300 SW Sixth Avenue, Suite 310, Portland OR 97201 U.S.A.

**GENERAL**

All fabrication shall take place in an enclosed factory environment by personnel experienced in the manufacture of outdoor site furniture.

**1. Materials**

Full-Round Log Seat shall be hand-hewn Douglas fir (Pseudo-tsuga menziesii), 22” dia. (+/- 2”), peeled of bark, sanded and saw kerfed full length. Ends shall be chamfered. Seat shall be anchored using provided 5/8” dia. x 14” hot dipped galvanized lag screws.

**2. Construction**

Log Seat shall be peeled by hand. *Logs that have been machine peeled or that include bark will not be accepted.* To effectively receive pressure preservative treatment, all fabrication, including sawing and drilling must be completed prior to preservative treatment. To resist seasoning checks, seat must include a full length saw kerf extending from the center of the log to the downward face.

**3. Finish**

Full-Round Steppers shall be pressure treated with a non-toxic child safe preservative after all fabrication is completed. *Preservatives containing arsenic, pentachlorophenol, creosote or similar toxic chemicals as their active ingredient shall not be used.*