**No. 2215TimberCraft***®* **Half-Round Log Seat**

Half-Round Log Seat shall be TimberCraft*®* series model No. 2215, in the length and quantity shown on the bill of materials or the project drawings. Manufacturer, Columbia Cascade Company, 1300 SW Sixth Avenue, Suite 310, Portland OR 97201 U.S.A.

**GENERAL**

All fabrication shall take place in an enclosed factory environment by personnel experienced in the manufacture of outdoor site furniture.

**1. Materials**

Log Seat shall be hand-hewn coastal Douglas fir (Pseudo-tsuga menziesii), 20” dia. (+/- 2”), peeled of bark and sanded. Edges and ends shall be chamfered. Seat shall be attached to bases with ½” dia. x 10” hot dipped galvanized lag screws. Base shall be hand-hewn coastal Douglas fir (Pseudo-tsuga menziesii), 9” dia. x 1’-8” peeled of bark and sanded.

**2. Construction**

Log Seat shall be peeled by hand. *Logs that have been machine peeled or that include bark will not be accepted.* To effectively receive pressure preservative treatment, all fabrication, including sawing and drilling must be completed prior to preservative treatment.

**3. Finish**

Seat shall be pressure treated with a non-toxic child safe preservative after all fabrication is completed. *Preservatives containing arsenic, pentachlorophenol, creosote or similar toxic chemicals as their active ingredient shall not be used.*